**LR 02-A** (1953) **Muir Hill Site Dumper**

|  |  |  |
| --- | --- | --- |
| © year on base: nonescale: 1:93 (not cast on base)length: 42mmwidth: 23mmheight: 24mmMATCHBOX lettering on base: noneadditional lettering on base: nonecompany on base: LESNEY ENGLANDnumber on base: nonecast license plate: none | metal base is part of bodyno interiormetal driverno windowsmetal dump tilts |  |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **#** | **body / base** | **driver** | **front wheels** | **rear wheels** | **axles** | **deco** | **dump** | **dump hinge** | **sub-var** | **note** | **cate** | **area** | **Stannard #** | **Jones #** | **date** |
| 0010 | green E | brown | 8.5x12 **green** metal (no #) | 12.5x18 **green** metal | flat head crimped | gold grille | red | panel pin | ll | #2 |  |  | 01 | 01 | 1953 |
| 0020 | green E | brown | 8.5x12 **green** metal (no #) | 12.5x18 **green** metal | flat head crimped | gold grille | red | crimped round head pin |  | #2 |  |  | 02 | 02 | 1953 |
| 0030 | green E | brown | 8.5x12 unpainted metal (no #) | 12.5x18 unpainted metal | flat head crimped | gold grille | red | panel pin | ll | #2 |  |  | 03 | 03 | 1954 |
| 0040 | green E | brown | 8.5x12 unpainted metal (no #) | 12.5x18 unpainted metal | flat head crimped | gold grille | red | crimped round head pin | ll | #2 |  |  | 04 | 04 | 1954 |

**UK codes:**

|  |  |  |  |
| --- | --- | --- | --- |
| **02A** |  |  |  |

**SUB-VARIATIONS:**

| **code** | **front axle crimping side** | **rear axle crimping side** |
| --- | --- | --- |
| ll | crimped on left side | crimped on left side |
| lr | crimped on left side | crimped on right side |
| rl | crimped on right side | crimped on left side |
| rr | crimped on right side | crimped on right side |

**Previous ref.: none**

**Later ref.: none**

**BOX TYPES:**

| **#** | **type** | **description** | **note** | **area** | **date** |
| --- | --- | --- | --- | --- | --- |
| 01 | A | plain end flaps, without NEW MODEL, plain inner end flaps |  |  | 1953/54 |
| 02 | B1 | plain end flaps, without NEW MODEL, plain inner end flaps | same box also used for LR 02-B |  | 1955-57 |