**LR 08-A** (1954) **Caterpillar Tractor**

|  |  |  |
| --- | --- | --- |
| © year on base: nonescale: 1:137 (not cast on base)length: 41mmwidth: 28mmheight: 26mmMATCHBOX lettering on base: noneadditional lettering on base: nonecompany on base: LESNEY ENGLANDnumber on base: nonecast license plate: none | no basemetal driver is part of bodyno windowsrubber tracksmetal tow hook is part of body |  |

| **#** | **body** | **driver** | **grille** | **rollers** | **tracks** | **axles** | **engine** | **sub-var** | **note** | **cate** | **area** | **Stannard #** | **Jones #** | **date** |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 0010 | yellow E | **red**, black helmet | yellow | 9mm **yellow** metal | 24 tread green | flat head crimped | **fully open** | ll | #8 |  |  | 01 | 01 | 1954 |
| 0020 | yellow E | **red**, black helmet | yellow | 9mm **yellow** metal | 24 tread green | flat head crimped | closed at rear |  | #8 |  |  | 02 | 02 | 1954 |
| 0030 | yellow E | **red**, black helmet | yellow | 9mm unpainted metal | 24 tread green | flat head crimped | closed at rear |  | #8 |  |  | 03 | 03 | 1954 |
| 0040 | **lt.** yellow E | **red**, black helmet | **lt.** yellow | 9mm unpainted metal | 24 tread green | flat head crimped | closed at rear |  | #8 |  |  | 04 | 04 | 1954 |
| 0050 | **orange** E | orange, black helmet | **gold** | 9mm unpainted metal | 24 tread green | flat head crimped | closed at rear | ll, rr | #8 |  |  | 05 | 05 | 1955 |
| 0060 | **orange** E | orange, black helmet | **gold** | 9mm unpainted metal | 24 tread green | flat head crimped | **closed at upper front and rear** | ll, [rr] | #8 |  |  | 06 | 06 | 1955 |
| 0070 | yellow E | yellow, black helmet | silver | 9mm unpainted metal | 24 tread green | flat head crimped | **closed at upper front and rear** | rr | #8 |  |  | 07 | 07 | 1955 |
| 0080 | yellow E | yellow, black helmet | silver | 9mm unpainted metal | 24 tread green | flat head crimped | fully closed | ll | #8 |  |  | 08 | 08 | 1957 |
| 0090 | **lt.** yellow E | **lt.** yellow, black helmet | silver | 9mm unpainted metal | 24 tread green | flat head crimped | fully closed | [rr] | #8 |  |  |  |  | 1957 |
| 0100 | yellow E | yellow, black helmet | **yellow** | 9mm unpainted metal | 24 tread green | flat head crimped | fully closed |  | #8 |  |  | 09 | 09 | 1957 |
| 0110 | yellow E | yellow, black helmet | **yellow** | 9mm unpainted metal | 24 tread **gray** | flat head crimped | fully closed |  | #8 |  |  | 10 | 10 | 1957 |

**UK codes:**

|  |  |  |  |
| --- | --- | --- | --- |
| **08A** |  |  |  |

**NOTE:**

**Same body as LR 18-A.**

**SUB-VARIATIONS:**

| **code** | **front axle crimping side** | **rear axle crimping side** |
| --- | --- | --- |
| ll | crimped on left side | crimped on left side |
| lr | crimped on left side | crimped on right side |
| rl | crimped on right side | crimped on left side |
| rr | crimped on right side | crimped on right side |

**Previous ref.: none**

**Later ref.: none**

**BOX TYPES:**

| **#** | **type** | **description** | **note** | **area** | **date** |
| --- | --- | --- | --- | --- | --- |
| 01 | B1 | plain end flaps, without NEW MODEL, without "REG.D", plain inner end flaps |  |  | 1954/55 |
| 02 | B1 | plain end flaps, without NEW MODEL, with "REG.D", plain inner end flaps |  |  | 1956 |
| 03 | B2 | small picture, side view shown, black number, no model name, without NEW MODEL, plain inner end flaps | same box also used for LR 08-B |  | 1957 |
| 04 | B2 | large picture, side view shown, black number, no model name, without NEW MODEL, plain inner end flaps | same box also used for LR 08-B |  | 1957 |
| 05 | B2 | front view shown, black number, no model name, without NEW MODEL, plain inner end flaps | same box also used for LR 08-B |  | 1957 |