**LR 16-A** (1955) **Transporter Trailer**

|  |  |  |
| --- | --- | --- |
| © year on base: none  scale: 1:162 (not cast on base)  length: 74/80mm  width: 26mm  height: 12mm  MATCHBOX lettering on base: none  additional lettering on base: none  company on base: LESNEY ENGLAND  number on base: none  cast license plate: none | metal base is part of body  no interior  no windows  metal tow bar tilts  metal ramp tilts |  |

| **#** | **body / base** | **wheels** | **axles** | **deco** | **tow bar** | **trailer ramp** | **ejector post** | **sub-var** | **note** | **cate** | **area** | **Stannard #** | **Jones #** | **date** |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 0010 | lt. brown E | 7x18 unpainted metal (no #) | flat head crimped | none | lt. brown | **thin** center, **no** posts | **plain ejector post** | lll | #16 |  |  | 01 | 01 | 1955 |
| 0020 | lt. brown E | 7x18 unpainted metal (no #) | flat head crimped | none | lt. brown | thickened center, **no** posts | **with build up to the front** | lll | #16 |  |  | 02 | 02 | 1955 |
| 0030 | lt. brown E | 7x18 unpainted metal (no #) | flat head crimped | none | lt. brown | thickened center, **no** posts | with build up & collar |  | #16 |  |  |  | 03 | 1955 |
| 0035 | lt. brown E | 7x18 unpainted metal (no #) | **dome** head crimped | none | lt. brown | thickened center, **no** posts | with build up & collar | (lll) | #16 |  |  |  |  | 1957 |
| 0040 | lt. brown E | 7x18 unpainted metal (no #) | flat head crimped | none | lt. brown | thickened center, with posts | with build up & collar | lll, rrr | #16 |  |  | 03 | 04 | 1956 |
| 0050 | lt. brown E | 7x18 unpainted metal (no #) | **dome** head crimped | none | lt. brown | thickened center, with posts | with build up & collar | lll | #16 |  |  | 04 | 05 | 1957 |
| 0060 | **med.** brown E | 7x18 unpainted metal (no #) | flat head crimped | none | **med.** brown | thickened center, with posts | with build up & collar |  | #16 |  |  |  | 06 | 1957 |
| 0070 | **med.** brown E | 7x18 unpainted metal (no #) | **dome** head crimped | none | **med.** brown | thickened center, with posts | with build up & collar | (lll) | #16 |  |  |  | 07 | 1957 |

**UK codes:**

|  |  |  |  |
| --- | --- | --- | --- |
| **16A** |  |  |  |

**SUB-VARIATIONS:**

| **code** | **first axle crimping side** | **second axle crimping side** | **third axle crimping side** |
| --- | --- | --- | --- |
| lll | crimped on left side | crimped on left side | crimped on left side |
| llr | crimped on left side | crimped on left side | crimped on right side |
| lrl | crimped on left side | crimped on right side | crimped on left side |
| lrr | crimped on left side | crimped on right side | crimped on right side |
| rll | crimped on right side | crimped on left side | crimped on left side |
| rlr | crimped on right side | crimped on left side | crimped on right side |
| rrl | crimped on right side | crimped on right side | crimped on left side |
| rrr | crimped on right side | crimped on right side | crimped on right side |

**Previous ref.: none**

**Later ref.: none**

**BOX TYPES:**

| **#** | **type** | **description** | **note** | **area** | **date** |
| --- | --- | --- | --- | --- | --- |
| 01 | B1 | very narrow, plain end flaps, without NEW MODEL, plain inner end flaps |  |  | 1955 |
| 02 | B1 | blurred picture, narrow, plain end flaps, without NEW MODEL, plain inner end flaps |  |  | 1955 |
| 03 | B1 | sharp picture, narrow, plain end flaps, without NEW MODEL, plain inner end flaps |  |  | 1956 |
| 04 | B2 | solid tow bar shown, black number, no model name, without NEW MODEL, plain inner end flaps |  |  | 1957 |
| 05 | B2 | outlined tow bar shown, black number, no model name, without NEW MODEL, plain inner end flaps |  |  | 1957 |
| 06 | B3 | black number in white circle, no model name, without NEW MODEL, plain inner end flaps | same box also used for LR 16-B |  | 1958/59 |