**LR 72-B** (1966) **JEEP (CJ 5)**

|  |  |  |
| --- | --- | --- |
| © year on base: none  scale: 1:63 (not cast on base)  length: 61mm  width: 31mm  height: 30mm  MATCHBOX lettering on base: straight  additional lettering on base: none  company on base: MADE IN ENGLAND BY LESNEY  number on base: 72  cast license plate: none | metal base  plastic interior  no window glazing  plastic wheels & tires  dome head rounded axles  plastic tow hook is part of interior  spare tire at rear |  |

| **#** | **body** | **base** | **interior** | **wheels** | **tires** | **deco** | **hood post** | **tow hook** | **grille inside** | **sub-var** | **note** | **cate** | **area** | **Stannard #** | **Jones #** | **date** |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 0010 | **lt.** yellow | gloss black E | **white** | 8mm yellow | 14x72 black | none | **no** | **2**mm **short** | smooth |  | #72 |  |  |  |  | 1966 |
| 0020 | med. yellow | gloss black E | **white** | 8mm yellow | 14x72 black | none | **no** | **2**mm **short** | smooth |  | #72 |  |  |  | 04 | 1966 |
| 0030 | **lt.** yellow | gloss black E | red | 8mm yellow | 14x72 black | none | **no** | **2**mm **short** | smooth | x | #72 |  |  |  |  | 1966 |
| 0040 | med. yellow | gloss black E | red | 8mm yellow | 14x72 black | none | **no** | **2**mm **short** | smooth | x | #72 |  |  | 01 | 01 | 1966 |
| 0050 | med. yellow | gloss black E | red | 8mm yellow | 14x72 black | none | yes | 3mm long | smooth | x | #72 |  |  | 02 | 02 | 1967 |
| 0060 | med. yellow | **flat** black E | red | 8mm yellow | 14x72 black | none | yes | 3mm long | smooth | x | #72 |  |  |  | 03 | 1969 |
| 0065 | **lt.** yellow | **flat** black E | red | 8mm yellow | 14x72 black | none | yes | 3mm long | smooth | (x) | #72 |  |  |  |  | 1969 |
| 0070 | med. yellow | gloss black E | red | 8mm yellow | 14x72 black | none | yes | 3mm long | **raised panel** |  | #72 |  |  |  | 06 | 1969 |
| 0080 | med. yellow | **flat** black E | red | 8mm yellow | 14x72 black | none | yes | 3mm long | **raised panel** |  | #72 |  |  |  |  | 1969 |
| 0090 | **dk.** yellow | gloss black E | red | 8mm yellow | 14x72 black | none | yes | 3mm long | smooth |  | #72 |  |  |  | 05 | 1967 |
| 0100 | **dk.** yellow | **flat** black E | red | 8mm yellow | 14x72 black | none | yes | 3mm long | smooth | x | #72 |  |  |  |  | 1969 |
| 0110 | **dk.** yellow | gloss black E | red | 8mm yellow | 14x72 black | none | yes | 3mm long | **raised panel** |  | #72 |  |  |  |  | 1969 |
| 0120 | **dk.** yellow | **flat** black E | red | 8mm yellow | 14x72 black | none | yes | 3mm long | **raised panel** |  | #72 |  |  |  |  | 1969 |
| 0130 | **orange-**yellow | gloss black E | red | 8mm yellow | 14x72 black | none | yes | 3mm long | **raised panel** | x | #72 |  |  |  |  | 1970 |

**UK codes:**

|  |  |  |  |
| --- | --- | --- | --- |
| **72B** |  |  |  |

**NOTE:**

**Rear panel casting with low horizontal line, rivets in tailgate hinge.**

**Previous ref.: none**

**Later ref.: ⇒ ⇒ ⇒ LS 72-A JEEP (CJ 5)**

**BOX TYPES:**

| **#** | **type** | **description** | **note** | **area** | **date** |
| --- | --- | --- | --- | --- | --- |
| 01 | E4 | light blue sides, color picture with "MATCHBOX" on end flaps, with NEW MODEL, no ®, flags on inner end flaps |  |  | 1966 |
| 02 | E4 | light blue sides, color picture with "MATCHBOX" on end flaps, without NEW MODEL, no ®, flags on inner end flaps |  |  | 1967 |
| 03 | E4 | light blue sides, color picture with "MATCHBOX" on end flaps, without NEW MODEL, ®, flags on inner end flaps |  |  | 1968 |
| 04 | F | without NEW, A LESNEY PRODUCT, no trademark on end flaps, no MARK on end flaps |  |  | 1969/70 |