**LS 44-A** (1970) **G.M.C. REFRIGERATOR TRUCK**

|  |  |  |
| --- | --- | --- |
| © year on base: nonescale: 1:94 (not cast on base)length: 76mmwidth: 29mmheight: 37mmMATCHBOX lettering on base: straightadditional lettering on base: SUPERFAST (straight)company on base: LESNEYnumber on base: 44cast license plate: none | metal containermetal chassis is part of body(A) at rear of basePAT APP at rear of basetow guideno interiorblack plastic wheels with silver hubsgray plastic rear door openswith rear door stop and rear bumpershort single removable plastic axle covers |  |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **#** | **body / chassis** | **container** | **grille / cab base** | **windows** | **wheels** | **deco** | **axle covers** | **sub-var** | **note** | **cate** | **area** | **Mack #** | **Mack date** | **date** |
| 01 | **red** E | **turquoise** | gray plastic | green | 4 spoke 11.5x2mm | none | black | f | #44 |  |  | 01 |  | 1970 |
| 06 | yellow E | **turquoise** | gray plastic | green | 4 spoke 11.5x2mm | none | black |  | #44 |  |  | 06 | 1993-03 | 1970 |
| 02 | yellow E | red | gray plastic | green | 4 spoke 11.5x2mm | none | black | f, r | #44 |  |  | 02 |  | 1970 |
| 04 | yellow E | red | gray plastic | green | 4 spoke 11.5x2mm | none | **red** | f, r | #44 |  |  | 04 |  | 1970 |
| f01 | yellow E | red | gray plastic | green | 4 spoke 11.5x2mm front,4 spoke 11.5x**4**mm rear | none | black |  | #44 |  |  |  |  | 1971 |
| 03 | yellow E | red | gray plastic | green | 4 spoke 11.5x**4**mm | none | black | f | #44 |  |  | 03 |  | 1971 |
| 05 | yellow E | red | gray plastic | green | 4 spoke 11.5x**4**mm | none | **red** |  | #44 |  |  | 05 |  | 1971 |

**USA codes:**

|  |  |  |  |
| --- | --- | --- | --- |
| **MB 44-A** |  |  |  |

**UK codes:**

|  |  |  |  |
| --- | --- | --- | --- |
| **44C** |  |  |  |

|  |  |
| --- | --- |
| **ROW numbers:** | **44** (1970-1971) |
| **USA numbers:** | **44** (1970-1971) |
| **Other numbers:** | **none** |

**NOTES:**

**Rear doors come with varying die numbers from 1 to 10.**

**Gray rear doors are prone to fading to gray-brown.**

**SUB-VARIATIONS:**

| **code** | **panel at container front** |
| --- | --- |
| f | flat |
| r | raised |

**Previous ref.: ⇒ ⇒ ⇒ LR 44-C G.M.C. REFRIGERATOR TRUCK**

**Later ref.: none**

**BOX TYPES:**

| **#** | **type** | **description** | **note** | **area** | **date** |
| --- | --- | --- | --- | --- | --- |
| 01 | G | with NEW, red TM, "MATCHBOX" REG'D T.M. ..., SF parallel on sides, MARK 3 on end flaps, no SPECIFICATION... on end flaps |  |  | 1970 |
| 02 | G | with NEW, black TM, "MATCHBOX" REG'D T.M. ..., SF angled on sides, MARK 4 on end flaps, no SPECIFICATION... on end flaps |  |  | 1971 |
| 03 | G | with NEW, no TM, "MATCHBOX" REG'D T.M. ..., SF angled on sides, MARK 4 on end flaps, no SPECIFICATION... on end flaps |  |  | 1971 |