**LS 48-D** (1981) **RED RIDER**

|  |  |  |
| --- | --- | --- |
| © year on base: 1972scale: 1:64 (not cast on base)length: 75mmwidth: 36mmheight: 36mmMATCHBOX lettering on base: bold italic / bold italic in frameadditional lettering on base: Superfast (script) / nonecompany on base: LESNEY PROD. & CO. LTD (Hong Kong) / LESNEY PRODUCTS PLC (England)number on base: 48 / nonecast license plate: none | metal baseno interiorblack plastic wheels with silver hubssilver plated plastic engine with silver stacksplastic grille & side exhausts |  |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **#** | **body** | **base** | **windows** | **front wheels** | **rear wheels** | **deco** | **grille / exhausts** | **sub-var** | **note** | **cate** | **area** | **Mack #** | **Mack date** | **date** |
| 01 | red | flat black **Ho** | red | malt. cross 12x6.5mm | malt. cross 16x9mm | white RED RIDER tampo | black | x | #48 |  | USA | 01 |  | 1981 |
| 04 | red | gloss black E | red | malt. cross 12x6.5mm | malt. cross 16x9mm | white RED RIDER tampo | black |  | #48 |  | USA | 04 |  | 1982 |
| 02 | red | **matt** black E | red | malt. cross 12x6.5mm | malt. cross 16x9mm | white RED RIDER tampo | black |  | #48 |  | USA | 02 |  | 1982 |
| 05 | red | gloss black E | red | malt. cross 12x6.5mm | malt. cross 16x9mm | white RED RIDER tampo | **dk. gray** |  | #48 |  | USA | 05 |  | 1982 |
| 03 | red | **matt** black E | red | malt. cross 12x6.5mm | malt. cross 16x9mm | white RED RIDER tampo | **dk. gray** |  | #48 |  | USA | 03 |  | 1982 |
| 11 | red | gloss black E | red | malt. cross 12x6.5mm | **5 crown** 16x9mm | white RED RIDER tampo | black | x | #48 |  | USA | 11 | 1984-06 | 1982 |
| 12 | red | **matt** black E | red | malt. cross 12x6.5mm | **5 crown** 16x9mm | white RED RIDER tampo | black |  | #48 |  | USA | 12 | 1984-06 | 1982 |
| f01 | red | gloss black E | red | **5 crown** 11.5x6.5mm | **5 crown** 16x9mm | white RED RIDER tampo | black |  | #48 |  | USA |  |  | 1982 |
| f02 | red | gloss black E | red | malt. cross 12x6.5mm | malt. cross 16x9mm | white flames, **no side tampo** | black |  | #48 |  | USA |  |  | 1982 |

**USA codes:**

|  |  |  |  |
| --- | --- | --- | --- |
| **MB 48-D** |  |  |  |

**UK codes:**

|  |  |  |  |
| --- | --- | --- | --- |
| **48D** |  |  |  |

|  |  |
| --- | --- |
| **ROW numbers:** | **none** |
| **USA numbers:** | **48** (1981-1982) |
| **Other numbers:** | **none** |

**NOTES:**

**Same body and windows as LS 26-B, LS 26-D and LS RN 07.**

**This model was allocated the MAN number 086 in 1982.**

**Previous ref.: ⇒ ⇒ ⇒ LS RN 03 WHITE LIGHTENING**

**Later ref.: ⇒ ⇒ ⇒ MI 086 RED RIDER**

**BOX TYPES:**

| **#** | **type** | **description** | **note** | **area** | **date** |
| --- | --- | --- | --- | --- | --- |
| 01 | L-USA | with NEW, "MATCHBOX" IS THE REGISTERED..., one line in rectangle, MARK on end flaps, no circled cross on inner end flaps |  | USA | 1981 |
| 02 | M | red & yellow generic picture box |  | USA | 1982 |